{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":89,"n_cols":7,"rows_kept":89,"merged":[[0,0,0,6],[14,1,17,1],[21,1,22,1],[23,1,24,1],[23,2,24,2],[48,1,49,1],[48,3,49,3],[53,1,58,1],[53,2,54,2],[55,2,56,2],[57,2,58,2],[59,1,60,1],[59,2,60,2],[88,0,88,6]]}
["宣传广告制品参考清单"]
["序号","内容","材质","规格型号","单位","报价","备注"]
["1","会议桌签","300g铜版纸内页","19cm*10cm","张"]
["2","玻璃腰线","户外防水车贴+UV喷印","1*0.15","m"]
["3","吊牌","拉丝钛金不锈钢吊牌+防水腐蚀字工艺","2.5m*0.35m","块"]
["4","食堂文化宣传","亚克力板，晶片uv打印，雕刻","0.6*0.9","块"]
["5","袖标","平绒布+发泡印","14cm宽×40cm","个"]
["6","反光袖标","三角联肩袖标，专用布料，反光字，魔术贴，定做",null,"个"]
["7","志愿者马甲及印字","马甲，制版，丝网印制",null,"件"]
["8","劳动竞赛旗","高档龙须平绒布，专版印制，挂坠","0.5*0.4","面"]
["9","意见箱","透明彩贴+箱体","34cm×25cm×13cm","个"]
["10","员工工作牌","PVC板（双面圆角+挂绳）","7cm×12cm","个"]
["11","纸杯","加厚+定制logo企业名称 ",null,"支"]
["12","科室牌","亚克力+uv+背喷","0.28m*0.15m","块"]
["13","岗位职责牌","户外写真+KT板+包银边","0.6m×0.8m","块"]
["14",null,"户外写真+pvc板+大银边","0.6m×0.8m","块"]
["15",null,"户外写真+pvc板+铝合金边","0.6m×0.8m","块"]
["16",null,"户外写真+pvc板+铝合金边+亚克力板","0.6m×0.8m","块"]
["17","宣传牌","8cm型材边，可开启式，高密板，uv打印，耐力板","2.4*1.2","块"]
["18","宣传牌","5cm型材边，可开启式，高密板，uv打印，耐力板","2.4*1.2","块"]
["19","亚克力盒子","白色亚克力背板，连接条，透明面板，无影胶粘接","21cm*30cm","个"]
["20","彩旗","旗帜布","0.6m×1.2m","面"]
["21",null,"旗杆（竹竿）","3m","根"]
["22","横幅","激光印（宽幅只有70cm/90cm）","70cm宽","m"]
["23",null,null,"90cm宽","m"]
["24","530喷绘","530喷绘","据实","㎡"]
["25","高精黑白加厚喷绘","高精度UV喷绘","据实","㎡"]
["26","旗台企业名称","铜版字",null,"cm"]
["27","旗帜（党旗、司旗）","丝绸彩印","3号旗","面"]
["28","不锈钢旗杆","114圆管、89圆管、76圆管、圆球、拉绳、转接头、滑轮",null,"m"]
["29","发光字","冲孔字+镀锌板+激光穿孔+防雨LED灯+烤漆","据实","cm"]
["30","铁皮字","镀锌板+激光焊接+烤漆",null,"cm"]
["31","箱体字","镀锌板+激光焊接+烤漆",null,"㎡"]
["32","型材背景架","钢架+斜拉钢+型材扣板","据实","㎡"]
["33","不锈钢活动展板","φ63mm圆管+30mm×50mm方钢管+氩弧焊接","1.2m×2.4m","块"]
["34","型材展板","φ63mm圆管+38mm×58mm方钢管+氩弧焊接","1.2m×2.4m","块"]
["35","报刊展台板","方通，烤漆，雨棚","1.2m×2.4m","块"]
["36","形象墙","木龙骨架+木工板底+铝塑板+蓝色干挂板","据实","㎡"]
["37","uv字","15+3雕刻",null,"cm"]
["38","LED显示屏","全户外防水显示屏+WIFI控制",null,"㎡"]
["39","文化墙、党建制度",null,"据实","㎡"]
["40","常规无造型指路牌","80mm方管+30mm×40mm方钢管+铁皮+高光夜间反光膜","结合现场","㎡"]
["41","发光字造型指路牌","80mm方管+30mm×40mm方钢管+铝塑板+高密板字+发光字","1m×4m","块"]
["42","太阳能发光字供电系统","太阳能电池组，发光字供电，安装支架",null,"套"]
["43","吊牌","钛金+烤漆","0.3m×2m","个"]
["44","粉料罐喷字模具","镂空雕刻模具","单个字宽1.2m","个"]
["45","粉料罐喷字","喷漆","单个字宽1.2m","个"]
["46","留样盒","10mm亚克力板方形盒+推拉式","0.3m×0.3m×0.4m","个"]
["47","工地彩门","门式桁架+铁皮+喷绘布","净高、净宽应满足车辆通行（甲供混凝土、吊车）","㎡"]
["48",null,"造型彩门+铁皮+uv布",null,"㎡"]
["49","七牌一图、单位工程承建牌、宣传标语（单个字）等（带双支腿）","喷绘布+φ76mm圆管+30mm×40mm方钢管+1mm铁皮+挖坑+混凝土","2.0m×1.5m","㎡"]
["50","宣传海报","户外高精车贴+防水膜","0.6m×0.8m","张"]
["51","警示标识","高光反光膜","0.6m×0.8m","张"]
["52","警示标志牌","户外写真+KT板","0.6m×0.8m","块"]
["53",null,null,"1m*1m","㎡"]
["54",null,"户外写真+pvc板","0.6m×0.8m","块"]
["55",null,null,"1m*1m","㎡"]
["56",null,"户外写真+1mm铁皮","0.6m×0.8m","块"]
["57",null,null,"1m*1m","㎡"]
["58","安全警示牌","户外车贴+30mm×30mm方钢管+1mm铁皮","0.6m×0.8m","块"]
["59",null,null,"1m*1m","㎡"]
["60","安全制度牌","喷绘布+30mm+30mm方钢管","1m*1m","㎡"]
["61","材料标识牌","钢架+铁皮+户外写真+覆膜+双立腿","0.3m*0.4m*1.2m","块"]
["62","分区牌","钢架+铁皮+户外写真+覆膜+双立腿","0.8m*0.6m*1.2m","块"]
["63","宣传手册、画册、汇报材料等","A4、B5纸+胶装","-","本"]
["64","交通标示牌","φ60mm圆钢管+铝板+高光夜间反光膜","φ60cm","套"]
["65","安全质量宣传标语","喷绘+30mm×30mm方钢管","1.5m*1.5m","块"]
["66","安全质量宣传标语","喷绘+30mm×30mm方钢管+铁皮","1.5m*1.5m","块"]
["67","宣传牌、五牌一图等（双支腿）","喷绘+30mm镀锌管加+铁皮+φ76圆管+双立柱","1.5m×2m","㎡"]
["68","联体五牌一图、宣传牌","喷绘+30mm镀锌管加+铁皮+φ76圆管+立柱+角钢+不锈钢边","结合现场","m2"]
["69","龙骨架标语","角钢+铁皮+喷绘+基础+龙骨主体+混凝土","结合现场","m2"]
["70","活动式不反光警示牌","阜外高精车贴+覆膜+30mm镀锌管架+龙骨+活动式三角立牌","0.6m*1.2m*0.6m","块"]
["71","活动式反光警示牌","高光夜间反光膜+30mm镀锌管架+龙骨+活动式三角立牌","0.6m*1.2m*0.6m","块"]
["72","单立柱不反光警示牌","户外高精车贴+覆膜+30mm镀锌管架+龙骨+φ63圆管+单立柱","0.6m*1m*3m","块"]
["73","单立柱反光警示牌","高光夜间反光膜+30mm镀锌管架+龙骨+φ63圆管+单立柱","0.6m*1m*3m","块"]
["74","爆闪单立柱反光警示牌","高光夜间反光膜+30mm镀锌管架+龙骨+φ63圆管+单立柱","0.8m*1m*3.5m","块"]
["75","便道广角镜","立杆，抱箍，混凝土，人工挖孔，凸透镜",null,"块"]
["76","限速牌","立杆，抱箍，混凝土，人工挖孔，凸透镜",null,"块"]
["77","隧道墙面导线标",null,"0.2m","m"]
["78","路面标线","反光标线",null,"m"]
["79","广告射灯","50Wled灯源",null,"个"]
["80","台车大功率防水广告投影灯","遥控款，防水，定制灯片，投射直径2m",null,"个"]
["81","效果图",null,null,"张"]
["82","vr效果图",null,null,"张"]
["83","火种收缴箱","亚克力，uv打印，亚克力箱体，滑槽，拉手，内部加筋加固","30cm*30cm*30cm","个"]
["84","不锈钢站位牌","不锈钢展架，pvc板，uv喷印","0.4*0.3*1.4","套"]
["85","中铁一局文化灯箱","高档磁吸，超薄灯箱，led灯带，高精灯片，uv打印，电源线",null,"块"]
["86","定做类配电箱防护棚","定制配电箱防护棚，焊接，防砸层，红白标线喷涂",null,"件"]
["注明：严格按照材质列表所要求的材质以及尺寸进行制作以及报价"]