{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":80,"n_cols":7,"rows_kept":80,"merged":[[0,0,0,6],[45,0,46,0],[45,1,46,1],[45,3,46,3],[45,4,46,4],[45,5,46,5],[45,6,46,6],[47,0,48,0],[47,1,48,1],[47,3,48,3],[47,4,48,4],[47,5,48,5],[47,6,48,6],[79,0,79,6]],"flags":["formulas_cached_only"]}
["宣传广告制品报价清单"]
["序号","内容","材质","规格型号","单位","报价","备注"]
[1,"二号旗","加厚户外防水织布","1.6m*2.4m","套"]
[2,"四号旗","加厚户外防水织布","1.44m*0.96m","套"]
[3,"玻璃腰线","户外防水车贴+UV喷印","1m*0.12m","平方米"]
[4,"会议桌签","5mm厚亚克力型材+300g铜版纸内页","25cm*10.2cm","套"]
[5,"食堂文化宣传","5cm铝合金边框+KT板+高清户外写真UV喷印+耐力板","90cm*60cm","套"]
[6,"陕西特色食品宣传","5cm铝合金边框+KT板+高清户外写真UV喷印+耐力板","1.76m*0.85m","套"]
[7,"项目部展板","5cm铝合金边框+KT板+高清户外写真UV喷印+耐力板","2.4m*1.2m","套"]
[8,"洗手间节约及爱护卫生宣传","5mm结皮板+高清UV喷印","24cm*12cm","块"]
[9,"门牌","4cm后铝合金型材+户外高清UV喷印+覆膜","28cm*21cm","块"]
[10,"电梯楼层牌","5mm亚克力+高清背面喷印","50cm*25cm","块"]
[11,"项目部门口钛金字","5cm厚加厚拉丝钛金","4.5m*0.3m","平方米"]
[12,"项目部会议室雕刻字","1cm厚结皮板激光雕刻","5.25m*0.3m","平方米"]
[13,"项目部门头发光字","8cm厚不锈钢包边+亚克力面板+防水背板+高亮度灯带","1.75m*1.8m","平方米"]
[14,"钢架+铁皮","30方管+1mm厚铁皮","1m*1m","平方米"]
[15,"茶杯","301ML中式陶瓷茶杯+托盘","301ML","套"]
[16,"纸杯","加厚+定制logo企业名称","9盎司","个"]
[17,"抽纸盒","皮质+定制logo企业名称","15cm*10cm","套"]
[18,"吊牌","拉丝钛金不锈钢吊牌+防水腐蚀字工艺","2m*0.4m","块"]
[19,"制度牌","5cm加厚铝合金边框+KT板+高清户外UV喷印写真","60cm*90cm","套"]
[20,"宿舍门牌","5mm后亚克力底板+高清UV背喷+双层加厚亚克力盒子","13cm*7.5cm","套"]
[21,"十二大理念展板","5cm加厚铝合金边框+KT板+高清户外UV喷印写真","40cm*110cm","套"]
[22,"核心价值观理念展板","5cm加厚铝合金边框+KT板+高清户外UV喷印写真","0.7m*1.1m","套"]
[23,"工作理念展板","5cm加厚铝合金边框+KT板+高清户外UV喷印写真","0.7m*0.9m","套"]
[24,"接待室内宣传","5cm加厚铝合金边框+KT板+高清户外UV喷印写真","1.6m*0.8m","套"]
[25,"党的光辉历程展板","2cm结皮板底板+3mm亚克力UV背喷面板+1cm水晶字面板","1.2m*0.8m","平方米"]
[26,"项目部指引牌","40方管+2mm铁皮+1cm结皮板高清UV喷印+2cm结皮板雕刻字（双面）+100圆管支撑","6.5m高*1.5m宽","套"]
[27,"小心台阶提示","5mm厚结皮板+高清UV喷印","1.3m*0.14m","平方米"]
[28,"会议室墙","2cm木条打底龙骨+2mm铝塑板+高强度胶水+密封胶","13.8平方米","平方米"]
[29,"镂空字模","加厚铁皮+激光雕刻","1.2m*1.2m","平方米"]
[30,"拌合站刷罐","定制颜色漆+升降车+铁皮字模","5m*3m","平方米"]
[31,"试验室外墙16字方针","1cm结皮板+户外高清UV喷印","80cm*80cm","平方米"]
[32,"隧道口上方宣传","户外550加厚科宝布+高清UV喷印+30方管+1mm厚铁皮","28m*2.6m","平方米"]
[33,"拌合站宣传牌（标识牌+合格仓）","30方管焊接+5mm结皮板+户外写真UV喷印+覆膜","50cm*70cm","块"]
[34,"拌合站水泥、粉煤灰标识牌","1cm厚户外结皮板+高清UV喷印","3.3m*1.65m","平方米"]
[35,"钢筋棚内宣传","户外550加厚科宝布+高清UV喷印+30方管焊接","80m*2.5m","平方米"]
[36,"便道反光条","加厚户外反光贴+高清UV喷印","1.2m*0.8m","平方米"]
[37,"便道行车安全警示牌","30方管边框+1mm铁皮+80圆管支撑+KT板+户外高清UV反光贴","1.2m*0.8m","套"]
[38,"道路冰雪注意安全提示牌","40方管边框+1mm铁皮+80圆管支撑+KT板+户外高清UV反光贴","1.8m*1.2m","套"]
[39,"国标广角镜","广角镜+立杆","0.8*3m","套"]
[40,"LED屏（户外）","P10高清户外专用LED屏","根据现场实际尺寸","平方米"]
[41,"LED屏（户外）","P3高清户外专用全彩LED屏","根据现场实际尺寸","平方米"]
[42,"钢筋棚外墙项目名称","10cm厚铁皮烤漆字+吊车安装+字模","1.5m*1.5m","平方米"]
[43,"钢筋棚侧墙宣传","1cm结皮板+户外高清UV喷印+30方管架子","4m*2m","套"]
[44,"不锈钢架子宣传栏","1cm厚结皮板+UV高清喷印+63不锈钢管1mm厚+","4m*1.2m","套"]
[null,null,"加厚亚克力雨棚+40不锈钢管+焊接处喷漆"]
[45,"不锈钢架子宣传栏","1cm厚结皮板+UV高清喷印+63不锈钢管2mm厚+","2.4m*1.2m","套"]
[null,null,"加厚亚克力雨棚+40不锈钢管+焊接处喷漆"]
[46,"党员示范岗","加厚亚克力背喷","19cm*13cm","套"]
[47,"刀旗","旗帜布+热转印+缝制+竹子旗杆","3m竹竿+55cm*120cm旗","套"]
[48,"会议室T型旗","平杆+高密度织布旗帜","32.5cm*27.5cm","套"]
[49,"投票箱","加厚亚克力+高清uv背喷","50cm*30cm*30cm","个"]
[50,"工地试验室楼顶广告","40方管焊架+铁皮烤漆字","60cm*70cm","平方米"]
[51,"横幅","高密度防水户外横幅","70cm高长度根据现场尺寸","米"]
[52,"岗位职责","5cm铝合金边框+KT板+高清户外写真UV喷印+耐力板","60cm*90cm","套"]
[53,"平面图，隧道纵断面图","5cm铝合金边框+KT板+高清户外写真UV喷印+5mm耐力板","3.5m*1.2m","套"]
[54,"办公室工程遮光窗帘","全遮光pvc 涤纶+定制logo企业名称","3.3m*1.4m","平方米"]
[55,"晴雨表","1cm结皮板+高清UV车贴+覆膜","90cm*70cm","平方米"]
[56,"温湿度标识牌","户外写真+高清UV喷印","30cm*20cm","张"]
[57,"检验区标识牌","1cm厚结皮板+高清UV喷印","30cm*20cm","块"]
[58,"机械设备标识牌","户外车贴+高清UV喷印","40cm*30cm","张"]
[59,"配电箱标识牌","户外车贴+高清UV喷印","30cm*20cm","张"]
[60,"操作规程","户外车贴+高清UV喷印","40cm*30cm","张"]
[61,"罐车logo 企业名称","户外车贴+高清UV喷印","5.8平方米","平方米"]
[62,"宣誓牌","40方管+1cm结皮板uv","2.4m*1.2m","平方米"]
[63,"影像采集标识牌","白板UV","60cm*45cm","套"]
[64,"隧道围岩标识牌","5mmpvc写真覆膜","30cm20cm","块"]
[65,"前方施工，减速慢行标识牌","30方管打底+60圆管支撑+1mm双面铁皮+kt板+反光贴UV","1.2m*1m","套"]
[66,"消防卡","户外车贴+高清UV喷印+覆膜","15cm*10cm","张"]
[67,"森林防火宣传","1cm结皮板+高清uv喷印","2.4m*1.2m","块"]
[68,"爆破区警示牌","30方管+单面1mm铁皮+KT板+反光贴","80cm*60cm","套"]
[69,"袖标","加厚高密度织布+反光字体+定制企业logo名称","45cm*28cm","套"]
[70,"炸药库警示牌","30方管+单面铁皮+1cmpvc发光膜","2.5m*1.2m","块"]
[71,"应急物资库","1cm结皮板雕刻字","60cm","厘米"]
[72,"当心触电警示牌","30方管焊架+1cmpvc结皮板+高清uv喷印","1.1m*0.4m","套"]
[73,"安全警示镜架体","不锈钢焊接+打磨抛光+氩弧焊制（含镜子和宣传画面）","1.5*2.3m","套"]
[74,"车辆汇入减速慢行","30方管焊架，60圆管支撑，双面1mm铁皮，KT板，反光贴双面","3m*0.8m","套"]
[75,"便道口宣传","30方管制作框架+1mm铁皮+科宝布UV喷印","75m*2.5m","平方米"]
["注明：严格按照材质列表所要求的材质以及尺寸进行制作以及报价"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}