{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["报价表"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"报价表","index":0,"n_rows":58,"n_cols":6,"rows_kept":58,"merged":[[0,0,0,5],[1,0,1,5],[3,1,6,1],[7,1,10,1],[26,1,27,1],[28,1,29,1],[40,1,41,1],[52,1,55,1],[57,0,57,1]]}
["安全标识标牌报价表"]
["广告公司名称：                                      税率：                                        公章："]
["序号","项目名称","制作规格","单位","不含税单价/元","备注"]
[1,"球面钛金字制作安装（注安装视具体情况而定）","30cm以下","M"]
[2,null,"30cm-50cm","M"]
[3,null,"50cm-70cm","M"]
[4,null,"70cm-100cm","M"]
[5,"平面钛金字制作安装（注安装视具体情况而定）","30cm以下","M"]
[6,null,"30cm-50cm","M"]
[7,null,"50cm-70cm","M"]
[8,null,"70cm-100cm","M"]
[9,"简易不锈钢橱窗（墙内安全宣传栏）","通体不锈钢+喷绘，钻眼固定","M2"]
[10,"立式安全宣传栏","不锈钢框架+铝塑板底+户外写真，焊接腿脚","M2"]
[11,"喷绘广告布制作","户外加厚高精度喷绘布制作（550高密织布）/人工安装/胶水螺丝等辅料","M2"]
[12,"户外写真","户外车贴高精写真覆膜","M2"]
[13,"户外写真+KT板","户外高精写真裱KT板","M2"]
[14,"户外写真+KT板包银边","户外高精写真裱KT板包银边","M2"]
[15,"户外写真+3mmPVC","户外高精写真裱3mm雪弗板(PVC)","M2"]
[16,"户外写真+5mmPVC","户外高精写真裱5mm雪弗板(PVC)","M2"]
[17,"户外写真+ABS板","户外高精写真裱ABS板","M2"]
[18,"室内写真","户内背胶高精写真覆膜","M2"]
[19,"户内写真+KT板","户内写真+KT板","M2"]
[20,"户内写真+KT板包银边","户内写真+KT板包银边","M2"]
[21,"户内写真+3mmPVC","户内高精写真裱3mm雪弗板(PVC)","M2"]
[22,"户内写真+5mmPVC","户内高精写真裱5mm雪弗板(PVC)","M2"]
[23,"亚克力安全宣传展板","高精写真裱5mm厚雪弗板+8mm透明有机玻璃(伸美牌国产精料)","M2"]
[24,"安全文化墙","0.8cmPVC附亚克力板Uv广告钉安装+雕刻","M2"]
[25,null,"PVC+雕刻","M2"]
[26,"LED广告屏","普通室外","M2"]
[27,null,"室内","M2"]
[28,"安全警示牌","高清户外车贴亮膜","M2"]
[29,"安全标识牌","高清户外车贴，镀锌方管焊接，镀锌板，双立柱","M2"]
[30,"红底黄字(白字)横幅宽1.2米","牛津布横幅","M"]
[31,"红底黄字(白字)横幅宽0.9米","牛津布横幅","M"]
[32,"安全讲话平台","背景板材质使用喷绘布， 周边外包框架，地面铺设草坪布","M2"]
[33,"安全警示镜","立柱采用不锈钢钢管， 面板采用不锈钢板","个"]
[34,"安全公示牌","25镀锌方管焊接框架表面加厚高精喷绘布","M2"]
[35,"警告标志","高清户外车贴，镀锌方管焊接，镀锌板（0.3*0.4M），立柱","M2"]
[36,"安全标志","可移动铝合金海报架","M2"]
[37,"玻璃门防撞条","塑料半透明磨砂贴背胶，宽 15cm，长=门宽，LOGO 及文字占幅宽 1/2 高度，上下各留空 1/4 高度。","M"]
[38,"安全宣传展板","材料：背板KT板，画面材料为背胶纸，根据具体情况覆亚膜或者亮膜，尺寸：0.6m×0.9m。","块"]
[39,null,"材料：背板KT板，画面材料为背胶纸，根据具体情况覆亚膜或者亮膜，尺寸：2.4m×1.2m。","块"]
[40,"限速牌","不锈钢管+彩色喷绘+KT板覆亚膜防水材质（0.25圆*0.25圆，墙面附着不锈钢管）","套"]
[41,"1km反光警示条、反光警示贴","/","M"]
[42,"灯箱","0.6*0.4m","M2"]
[43,"安全警戒标志","110圆管+警示牌(含立柱)","套"]
[44,"一个二级电箱防护罩","钢结构造型+钢结构框架+不锈钢包边+烤漆","M2"]
[45,"三角彩旗","经编布","M"]
[46,"警示柱","塑料","个"]
[47,"安全警示喷漆","/","M2"]
[48,"反光膜","/","M2"]
[49,"安全反光柱","110PVC圆管+晶彩格反光贴","套"]
[50,"安全警示牌","精彩格+烤漆板","M2"]
[51,"户外车贴","PVC户外不干胶","M2"]
[52,"制度牌亚克力UV","5mm亚克力uv","M2"]
[53,"PVC-UV","8毫米pvc-uv","M2"]
[54,"交通警示牌","30方管架子+60圆管+太阳能爆闪灯","套"]
["合 计（元）"]